Fire Safety Policy
The Yarcombe Jubilee Hall

The Yarcombe Jubilee Hall Management Committee has implemented the following to          ensure the fire safety of all users of The Yarcombe Jubilee Hall.
The Hall Officers are appointed the Fire Safety Co-ordinators and will keep a Fire Precautions Log Book.
All fire exits and escape routes are clearly signed and are required to be kept free of             obstructions at all times to ensure safe evacuation of the building.
All emergency lighting is checked on a monthly basis and serviced and maintained annually by an approved contractor and the results recorded.
Fire-fighting equipment is provided in appropriate places within the hall, according to the      particular fire risk posed.  All fire-fighting equipment will be visually checked on a monthly basis and will be serviced and maintained on an annual basis by an approved contractor and results recorded.  1 fire blanket and 5 fire extinguishers.
The hall electrical wiring installation is inspected every 5 years by an approved contractor and results recorded.  All portable electrical appliances, provided as hall facilities, are tested        annually by an approved contractor and the results recorded. The pressurised water heaters are serviced annually by an approved contractor and the results recorded.
The oil boiler is serviced annually and maintained by an approved contractor and the results recorded.
A Fire Risk Assessment is undertaken on at least an annual basis, and the results recorded. The Fire Risk Assessment will be a Standing Agenda item at all management meetings, to   ensure any additional Fire Risk Assessments are undertaken if any changes are made that may impact upon fire safety, such as alterations to the premises or new activities of hire.
All users of the hall will be required to familiarise themselves with the 'Fire Safety Guidance for Hirers and the Emergency Evacuation Plan' which is displayed on the premises.  
The Assembly Point is clearly signed, located top area of front car park.
Regular hall users will be advised that they should conduct formal fire evacuation drills for attendees.

Fire Safety Inspections
The Hall Officers will on behalf of Yarcombe Jubilee Hall Management Committee be responsible for conducting regular visual inspections of the hall premises and all its fire safety equipment.
           - All fire-fighting equipment is present and serviceable
           - All emergency lighting is working
           - All fire exits and escape routes are free of obstruction
           - Any flammable liquids are stored correctly
           - There is no accumulation of rubbish within or around the building.


Any committee members, hall hirers or attendees with concerns related to the fire safety of the hall must report to a Hall Officer immediately.
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